Thanks for purchasing PLANET GSD-1002M 8-Port 10/100/1000Mbps + 2-Port 100/1000X SFP Managed Desktop Switch.

This document provides the firmware release note and history of the products below:


Version v1.305b251017 Released on 20/10/2025
=======================================
Firmware version: v1.305b251017
Hardware version: 1.0
File Name: FW-GSD-1002M_v1.305b251017.bix
File Size: 6,736,357 bytes 
Released on 20/10/2025
=======================================

This firmware provides the following modifications:

A: Bug Fixed - NA

B:  Function Added - Support PLANET CloudNMS.  

C: Other - NA


[Upgrade procedure]:

1. Connect the RJ45 UTP cable to the target switch.

2. Login is required to access the Web interface after the booting is completed successfully. The factory default user name and password are both "admin".

3. When the Web UI main screen appears, click "Maintenance --> Upgrade Manager" on the left side of the Menu.  

4. The screen provides HTTP Firmware Upgrade and TFTP Firmware Upgrade.

   A. HTTP Firmware Upgrade
     (1) Use the "Browser" to locate firmware path.
     (2) Click the "Upgrade" button to start the firmware upgrade procedure. Please don't power off the switch while the procedure is starting.
     (3) Please wait until the system reboot is completed.
     (4) Reset to factory default and reboot system again.

   B. TFTP Firmware Upgrade

     (1) Enter the "TFTP Firmware Upgrade" and input TFTP Server IP address and filename with the correct firmware file.
     (2) Click the "Upgrade" button to start the firmware upgrade procedure. Please don't power off the switch while the procedure is starting.
     (3) Please wait until the successful message shows on the Update Status web page.
     (4) Please wait until the system reboot is completed.
     (5) Reset to factory default and reboot system again.

5. Relogin the switch via Web browser. Please click "System -->Management-->System Information --> Firmware Version" to double-check if the firmware is upgraded successfully.


******************************
Firmware Release History:  
******************************

Version v1.305b250121 Released on 05/02/2025
=======================================
Firmware version: v1.305b250121
Hardware version: 1.0
File Name: FW-GSD-1002M_v1.305b250121.bix
File Size: 6,658,933 bytes 
Released on 05/02/2024
=======================================

This firmware provides the following modifications:

A: Bug Fixed - NA

B: Functions added -Enhanced product security.   

C: Other - NA


=======================================
Version v1.305b240426 Released on 26/04/2024
=======================================
Firmware version: v1.305b240426
Hardware version: 1.0
File Name: FW-GSD-1002M_v1.305b240426.bix
File Size: 6,640,300 bytes 
Released on 26/04/2024
=======================================

This firmware provides the following modifications:

A: Bug Fixed - NA

B: Functions added - Added PSTI function   

C: Other - NA


=======================================
Version 1.305b210628 Released on 28/06/2021
=======================================
Firmware version: v1.305b210628
Hardware version: 1.0
File Name: FW-GSD-1002M_v1.305b210628.bix
File Size: 6,488,064 bytes 
Released on 28/06/2021
=======================================

This firmware provides the following modifications:

A: Bug Fixed - NA

B: Functions added - 
   (1) Added ERPS ring support.
   (2) Added enhanced cybersecurity support.
   (3) Added PLANET CloudViewer app and NMS controller support.
   (4) Supports SNMP LLDP MIB.   

C: Other -
   (1) Unified Web UI style.
   (2) HTTPs is enabled in the factory default mode.
   (3) Default Web login with HTTPs.

[Upgrade Requirements]:

1. The latest firmware version of GSD-1002M.
2. The GSD-1002M switch.
3. Workstation with Microsoft IE 8.0 or above.
4. TFTP server. (If you want to upgrade firmware via TFTP)

=======================================
Version 1.0b150211 Released on 11/02/2015
=======================================
Firmware version: v1.0b150211
Hardware version: 1.0
File Name: FW-GSD-1002M_v1.0b150211.bix
File Size: 5,754,880 bytes 
Released on 11/02/2015
=======================================


This firmware provides the following modifications:

A: Bug Fixed -
   (1) Fix SNMP configuration could not be saved after reboot.
   (2) Fix Removed dual image function.      
   
B. Function Added -
   (1) Added auto mode for SFP slots support.
   (2) Added PLANET Smart Discovery Lite support.  

C. Other:
   NA.

=======================================
Version 1.0b140225 Released on 25/02/2014
=======================================
Firmware version: v1.0b140225
Hardware version: 1.0
File Name: FW-GSD-1002M_v1.0b140225.bix
File Size: 5,713,920 bytes 
Released on  25/02/2014
=======================================


Initial Release.


Sincerely yours,
PLANET Technical Support Team
https://www.planet.com.tw


